پنجره ها

Construction,1002,

2;

Construction,2002,

2,

20034;

WindowProperty:ShadingControl,1002,

InteriorShade,

2002,

AlwaysOn,

,

,

No,

No,

,

FixedSlatAngle,

,

0;

Construction,1004,

2;

Construction,2004,

2,

20026;

Construction,1005,

2;

Construction,2005,

2,

20031;

Construction,1006,

2;

Construction,2006,

2,

20031;

WindowMaterial:Glazing,2,

SpectralAverage,

,

.003, thickness

.837, solar transmittance

.075, outside solar reflectance

.075, inside solar reflectance

.898, visible transmittance

.081, outside visible transmittance

.081, inside visible trasmittance

.0, infrared

.84, outside emissity

.84, inside emissity

.9, conductivity

1;

WindowMaterial:Glazing,3,

SpectralAverage,

,

.006,

.775,

.071,

.071,

.881,

.080,

.080,

.0,

.84,

.84,

.9,

1;

**تعاریف جدید**

**هوا ضخامت 10 میل**

WindowMaterial:Gas,1017,

Air,

.01;

WindowMaterial:Gas,Half thickness 1017,

Air,

.005;

گاز آرگون ضخامت 10 میل

WindowMaterial:Gas,1016,

Argon,

.010;

WindowMaterial:Gas,Half thickness 1016,

Argon,

.005;

شیشه ضخامت 4 میل

WindowMaterial:Glazing,63,

SpectralAverage,

,

.004,

.816,

.075,

.075,

0.892,

.081,

.081,

.0,

.84,

.84,

1,

1;

**پنجره 4+10+6 هوا**

Construction,1002,

63,

1017,

3;

Construction,2002,

63,

1017,

3,

20031;

Construction,2004,

63,

1017,

3,

20031;

Construction,1004,

63,

1017,

3;

**Cost= 1230000 t**

**پنجره 4+10+4 هوا**

Construction,1002,

63,

1017,

63;

Construction,2002,

63,

1017,

63,

20031;

Construction,2004,

63,

1017,

63,

20031;

Construction,1004,

63,

1017,

63;

**Cost=1100000 t**

**پنجره 4+10+6 آرگون**

Construction,1002,

63,

1016,

3;

Construction,2002,

63,

1016,

3,

20031;

Construction,2004,

63,

1016,

3,

20031;

Construction,1004,

63,

1016,

3;

**Cost= 1767000 t**

**پنجره 4+10+4 آرگون**

Construction,1002,

63,

1016,

63;

Construction,2002,

63,

1016,

63,

20031;

Construction,2004,

63,

1016,

63,

20031;

Construction,1004,

63,

1016,

63;

**Cost= 1557000 t**